CODDENHAM TREE SURVEY: MARCH 2023

SUMMARY OF PRIORITY OF WORKS – 2 year priority

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
|  | | | | | |
| **TREE LOCATION** | | **TREE #** | **PRIORITY** | | **SURVEY COMMENT & RECOMMENDATION** |
| Mill Hill | T5 | | 2 years | Field Maple: the top of the tree is dead.  **Recommend** coppice. | |
| Broom Hill | T8 | | 2 years | Common Oak: significant wound on north side of main stem. Lower wood is desiccated. Reactive callous growth present. Indicative decay extends down entire stem.  **Recommend** reduce tree height to ~10m where lateral branches have live buds. | |
| Broom Hill | T10 | | 2 years | Sycamore: potential stem failure. Tree targets footpath.  **Recommend** install dynamic fabric bracing system between 3 co-dominant stems. | |
| Broom Hill | T11 | | 2 years | Common Oak: tight union of co-dominant stems.  **Recommend** reduce the spread of the lateral limb on the north side by ~1.5m to reduce lever arm force. | |
| Broom Hill | T9 | | unspecified | Common Ash: significant dead wood and ivy in canopy.  **Recommend** reduce limb with apical dieback over footpath to ~8m. | |